
T5BD0 002:842 SEGGER J-Link V6.46 Log File (0001ms, 0003ms total)
T5BD0 002:842 DLL Compiled: May 23 2019 17:49:56 (0001ms, 0003ms total)
T5BD0 002:842 Logging started @ 2023-08-15 15:05 (0001ms, 0003ms total)
T5BD0 002:843 JLINK_SetWarnOutHandler(...) (0000ms, 0003ms total)
T5BD0 002:843 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled May  7 2021 16:26:12
Hardware: V9.40
S/N: 69407005
Feature(s): RDI, GDB, FlashDL, FlashBP, JFlash
TELNET listener socket opened on port 19021WEBSRV 
Starting webserver (0035ms, 0038ms total)
T5BD0 002:843 WEBSRV Webserver running on local port 19080 (0035ms, 0038ms total)
T5BD0 002:843   returns O.K. (0035ms, 0038ms total)
T5BD0 002:878 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0000ms, 0038ms total)
T5BD0 002:878 JLINK_TIF_GetAvailable(...) (0000ms, 0038ms total)
T5BD0 002:878 JLINK_SetErrorOutHandler(...) (0000ms, 0038ms total)
T5BD0 002:878 JLINK_ExecCommand("ProjectFile = "D:\Project\dtu\Bootloader\USER\JLinkSettings.ini"", ...). Ref file found at: D:\workSoftware\stm32Software\mdk\mdkcore\ARM\Segger\JLinkDevices.ref (0013ms, 0051ms total)
T5BD0 002:878 XML referenced by ref file: C:\Program Files (x86)\SEGGER\JLink\JLinkDevices.xml (0019ms, 0057ms total)
T5BD0 002:878 C:\Program Files (x86)\SEGGER\JLink\JLinkDevices.xml evaluated successfully.  returns 0x00 (0059ms, 0097ms total)
T5BD0 002:938 JLINK_ExecCommand("Device = GD32F103VG", ...). Device "GD32F103VG" selected.  returns 0x00 (0003ms, 0100ms total)
T5BD0 002:941 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 0100ms total)
T5BD0 002:941 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 0100ms total)
T5BD0 002:941 JLINK_GetDLLVersion()  returns 64600 (0000ms, 0100ms total)
T5BD0 002:942 JLINK_GetFirmwareString(...) (0000ms, 0101ms total)
T5BD0 002:946 JLINK_GetDLLVersion()  returns 64600 (0000ms, 0101ms total)
T5BD0 002:946 JLINK_GetCompileDateTime() (0000ms, 0101ms total)
T5BD0 002:947 JLINK_GetFirmwareString(...) (0000ms, 0101ms total)
T5BD0 002:948 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 0101ms total)
T5BD0 002:954 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0002ms, 0103ms total)
T5BD0 002:956 JLINK_SetSpeed(500) (0000ms, 0103ms total)
T5BD0 002:956 JLINK_GetId() >0x10B TIF>Found SW-DP with ID 0x1BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>Scanning AP map to find all available APs >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[1]: Stopped AP scan as end of AP map has been reachedAP[0]: AHB-AP (IDR: 0x24770011)Iterating through AP map to find AHB-AP to use
 >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[0]: Core foundAP[0]: AHB-AP ROM base: 0xE00FF000 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>CPUID register: 0x412FC231. Implementer code: 0x41 (ARM)Found Cortex-M3 r2p1, Little endian. -- Max. mem block: 0x00011028
 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88) -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)CoreSight components:ROMTbl[0] @ E00FF000
 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl[0][0]: E000E000, CID: B105E00D, PID: 000BB000 SCS -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl[0][1]: E0001000, CID: B105E00D, PID: 003BB002 DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0) -- CPU_ReadMem(16 bytes @ 0xE0002FE0)ROMTbl[0][2]: E0002000, CID: B105E00D, PID: 002BB003 FPB -- CPU_ReadMem(16 bytes @ 0xE0000FF0)
 -- CPU_ReadMem(16 bytes @ 0xE0000FE0)ROMTbl[0][3]: E0000000, CID: B105E00D, PID: 003BB001 ITM -- CPU_ReadMem(16 bytes @ 0xE00FF010) -- CPU_ReadMem(16 bytes @ 0xE0040FF0) -- CPU_ReadMem(16 bytes @ 0xE0040FE0)ROMTbl[0][4]: E0040000, CID: B105900D, PID: 003BB923 TPIU-Lite -- CPU_ReadMem(16 bytes @ 0xE0041FF0) -- CPU_ReadMem(16 bytes @ 0xE0041FE0)ROMTbl[0][5]: E0041000, CID: B105900D, PID: 003BB924 ETM-M3 >0x0D TIF> >0x21 TIF>  returns 0x1BA01477 (0188ms, 0291ms total)
T5BD0 003:144 JLINK_GetDLLVersion()  returns 64600 (0000ms, 0291ms total)
T5BD0 003:144 JLINK_CORE_GetFound()  returns 0x30000FF (0000ms, 0291ms total)
T5BD0 003:144 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0291ms total)
T5BD0 003:146 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 0291ms total)
T5BD0 003:146 JLINK_GetDebugInfo(0x101 = JLINKARM_DEBUG_INFO_ETM_ADDR_INDEX) -- Value=0xE0041000  returns 0x00 (0000ms, 0291ms total)
T5BD0 003:146 JLINK_ReadMemEx(0xE0041FD0, 0x0020 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(32 bytes @ 0xE0041FD0) - Data: 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0002ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x102 = JLINKARM_DEBUG_INFO_MTB_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x103 = JLINKARM_DEBUG_INFO_TPIU_ADDR_INDEX) -- Value=0xE0040000  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x104 = JLINKARM_DEBUG_INFO_ITM_ADDR_INDEX) -- Value=0xE0000000  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x105 = JLINKARM_DEBUG_INFO_DWT_ADDR_INDEX) -- Value=0xE0001000  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x106 = JLINKARM_DEBUG_INFO_FPB_ADDR_INDEX) -- Value=0xE0002000  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x107 = JLINKARM_DEBUG_INFO_NVIC_ADDR_INDEX) -- Value=0xE000E000  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x10C = JLINKARM_DEBUG_INFO_DBG_ADDR_INDEX) -- Value=0xE000EDF0  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_GetDebugInfo(0x01 = Unknown) -- Value=0x00000000  returns 0x00 (0000ms, 0293ms total)
T5BD0 003:148 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED00) - Data: 31 C2 2F 41  returns 1 (0001ms, 0294ms total)
T5BD0 003:149 JLINK_GetDebugInfo(0x10F = JLINKARM_DEBUG_INFO_HAS_CORTEX_M_SECURITY_EXT_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 0294ms total)
T5BD0 003:149 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 0294ms total)
T5BD0 003:149 JLINK_Reset() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET. >0x35 TIF>Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0093ms, 0387ms total)
T5BD0 003:242 JLINK_Halt()  returns 0x00 (0000ms, 0387ms total)
T5BD0 003:242 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) - Data: 03 00 03 00  returns 1 (0002ms, 0389ms total)
T5BD0 003:244 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0 (0001ms, 0390ms total)
T5BD0 003:245 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0 (0002ms, 0392ms total)
T5BD0 003:253 JLINK_GetHWStatus(...)  returns 0x00 (0001ms, 0393ms total)
T5BD0 003:257 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x06 (0000ms, 0393ms total)
T5BD0 003:257 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 0393ms total)
T5BD0 003:257 JLINK_GetNumWPUnits()  returns 0x04 (0000ms, 0393ms total)
T5BD0 003:261 JLINK_GetSpeed()  returns 0x1F4 (0000ms, 0393ms total)
T5BD0 003:263 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 02 00 00 00  returns 1 (0002ms, 0395ms total)
T5BD0 003:265 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 02 00 00 00  returns 1 (0001ms, 0396ms total)
T5BD0 003:266 JLINK_WriteMemEx(0xE0001000, 0x001C Bytes, ..., Flags = 0x02000004) - Data: 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ... -- CPU_WriteMem(28 bytes @ 0xE0001000)  returns 0x1C (0003ms, 0399ms total)
T5BD0 003:269 JLINK_Halt()  returns 0x00 (0000ms, 0399ms total)
T5BD0 003:269 JLINK_IsHalted()  returns TRUE (0000ms, 0399ms total)
T5BD0 003:275 JLINK_WriteMem(0x20000000, 0x01E8 Bytes, ...) - Data: 00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(488 bytes @ 0x20000000)  returns 0x1E8 (0018ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R0, 0x08000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R2, 0x00000001)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(R15 (PC), 0x20000038)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0417ms total)
T5BD0 003:293 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x00000001 (0002ms, 0419ms total)
T5BD0 003:295 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0025ms, 0444ms total)
T5BD0 003:320 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0018ms, 0462ms total)
T5BD0 003:338 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R0, 0x08000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R1, 0x00000800)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(R15 (PC), 0x20000020)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000002 (0000ms, 0444ms total)
T5BD0 003:338 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0016ms, 0460ms total)
T5BD0 003:354 JLINK_IsHalted()  returns FALSE (0001ms, 0461ms total)
T5BD0 003:378 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0017ms, 0477ms total)
T5BD0 003:395 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_ClrBPEx(BPHandle = 0x00000002)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R0, 0x08000800)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R1, 0x00000800)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0460ms total)
T5BD0 003:395 JLINK_WriteReg(R15 (PC), 0x20000020)  returns 0x00 (0001ms, 0461ms total)
T5BD0 003:396 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0461ms total)
T5BD0 003:396 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0461ms total)
T5BD0 003:396 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0461ms total)
T5BD0 003:396 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0461ms total)
T5BD0 003:396 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000003 (0000ms, 0461ms total)
T5BD0 003:396 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0015ms, 0476ms total)
T5BD0 003:411 JLINK_IsHalted()  returns FALSE (0001ms, 0477ms total)
T5BD0 003:415 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0018ms, 0494ms total)
T5BD0 003:433 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_ClrBPEx(BPHandle = 0x00000003)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R0, 0x00000001)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R1, 0x00000800)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(R15 (PC), 0x20000070)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000004 (0000ms, 0476ms total)
T5BD0 003:433 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0017ms, 0493ms total)
T5BD0 003:450 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0018ms, 0511ms total)
T5BD0 003:468 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0493ms total)
T5BD0 003:468 JLINK_ClrBPEx(BPHandle = 0x00000004)  returns 0x00 (0000ms, 0493ms total)
T5BD0 003:468 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0493ms total)
T5BD0 003:522 JLINK_WriteMem(0x20000000, 0x01E8 Bytes, ...) - Data: 00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(488 bytes @ 0x20000000)  returns 0x1E8 (0018ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R0, 0x08000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R2, 0x00000002)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(R15 (PC), 0x20000038)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0511ms total)
T5BD0 003:540 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x00000005 (0002ms, 0513ms total)
T5BD0 003:542 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0018ms, 0531ms total)
T5BD0 003:560 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0018ms, 0549ms total)
T5BD0 003:578 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0531ms total)
T5BD0 003:578 JLINK_ClrBPEx(BPHandle = 0x00000005)  returns 0x00 (0000ms, 0531ms total)
T5BD0 003:578 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0531ms total)
T5BD0 003:578 JLINK_WriteMem(0x200001E8, 0x0218 Bytes, ...) - Data: 10 10 00 20 4D 01 00 08 15 03 00 08 D7 02 00 08 ... -- CPU_WriteMem(536 bytes @ 0x200001E8)  returns 0x218 (0020ms, 0551ms total)
T5BD0 003:598 JLINK_WriteMem(0x20000400, 0x01E8 Bytes, ...) - Data: 80 25 C9 11 68 46 FF F7 AE FF C4 F3 09 02 29 46 ... -- CPU_WriteMem(488 bytes @ 0x20000400)  returns 0x1E8 (0017ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R0, 0x08000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R2, 0x200001E8)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(R15 (PC), 0x2000013C)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000006 (0000ms, 0568ms total)
T5BD0 003:615 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0017ms, 0585ms total)
T5BD0 003:632 JLINK_IsHalted()  returns FALSE (0000ms, 0585ms total)
T5BD0 003:639 JLINK_IsHalted()  returns FALSE (0001ms, 0586ms total)
T5BD0 003:642 JLINK_IsHalted()  returns FALSE (0001ms, 0586ms total)
T5BD0 003:645 JLINK_IsHalted()  returns FALSE (0001ms, 0586ms total)
T5BD0 003:648 JLINK_IsHalted()  returns FALSE (0002ms, 0587ms total)
T5BD0 003:651 JLINK_IsHalted()  returns FALSE (0001ms, 0586ms total)
T5BD0 003:654 JLINK_IsHalted()  returns FALSE (0001ms, 0586ms total)
T5BD0 003:657 JLINK_IsHalted()  returns FALSE (0001ms, 0586ms total)
T5BD0 003:660 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0017ms, 0602ms total)
T5BD0 003:677 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0585ms total)
T5BD0 003:677 JLINK_ClrBPEx(BPHandle = 0x00000006)  returns 0x00 (0000ms, 0585ms total)
T5BD0 003:677 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0585ms total)
T5BD0 003:677 JLINK_WriteMem(0x200001E8, 0x0218 Bytes, ...) - Data: 08 60 00 BF 2C 48 00 68 00 F0 02 00 00 28 F9 D0 ... -- CPU_WriteMem(536 bytes @ 0x200001E8)  returns 0x218 (0020ms, 0605ms total)
T5BD0 003:697 JLINK_WriteMem(0x20000400, 0x01E8 Bytes, ...) - Data: 01 2A 01 D1 00 2B F7 D1 01 2A 00 D1 04 22 10 46 ... -- CPU_WriteMem(488 bytes @ 0x20000400)  returns 0x1E8 (0018ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R0, 0x08000400)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R2, 0x200001E8)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(R15 (PC), 0x2000013C)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000007 (0000ms, 0623ms total)
T5BD0 003:715 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0017ms, 0640ms total)
T5BD0 003:732 JLINK_IsHalted()  returns FALSE (0001ms, 0641ms total)
T5BD0 003:736 JLINK_IsHalted()  returns FALSE (0001ms, 0641ms total)
T5BD0 003:739 JLINK_IsHalted()  returns FALSE (0001ms, 0641ms total)
T5BD0 003:742 JLINK_IsHalted()  returns FALSE (0001ms, 0641ms total)
T5BD0 003:745 JLINK_IsHalted()  returns FALSE (0002ms, 0642ms total)
T5BD0 003:750 JLINK_IsHalted()  returns FALSE (0002ms, 0642ms total)
T5BD0 003:753 JLINK_IsHalted()  returns FALSE (0002ms, 0642ms total)
T5BD0 003:756 JLINK_IsHalted()  returns FALSE (0001ms, 0641ms total)
T5BD0 003:759 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0017ms, 0657ms total)
T5BD0 003:776 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0640ms total)
T5BD0 003:776 JLINK_ClrBPEx(BPHandle = 0x00000007)  returns 0x00 (0000ms, 0640ms total)
T5BD0 003:776 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0640ms total)
T5BD0 003:776 JLINK_WriteMem(0x200001E8, 0x0218 Bytes, ...) - Data: 23 01 67 45 AB 89 EF CD E0 F7 FF 1F 70 B5 04 46 ... -- CPU_WriteMem(536 bytes @ 0x200001E8)  returns 0x218 (0021ms, 0661ms total)
T5BD0 003:797 JLINK_WriteMem(0x20000400, 0x01E8 Bytes, ...) - Data: 08 28 DE D3 08 20 22 E0 01 27 87 40 1F 40 E7 B1 ... -- CPU_WriteMem(488 bytes @ 0x20000400)  returns 0x1E8 (0018ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R0, 0x08000800)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R2, 0x200001E8)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(R15 (PC), 0x2000013C)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000008 (0000ms, 0679ms total)
T5BD0 003:815 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0016ms, 0695ms total)
T5BD0 003:831 JLINK_IsHalted()  returns FALSE (0002ms, 0697ms total)
T5BD0 003:835 JLINK_IsHalted()  returns FALSE (0001ms, 0696ms total)
T5BD0 003:838 JLINK_IsHalted()  returns FALSE (0001ms, 0696ms total)
T5BD0 003:841 JLINK_IsHalted()  returns FALSE (0001ms, 0696ms total)
T5BD0 003:844 JLINK_IsHalted()  returns FALSE (0001ms, 0696ms total)
T5BD0 003:847 JLINK_IsHalted()  returns FALSE (0001ms, 0696ms total)
T5BD0 003:850 JLINK_IsHalted()  returns FALSE (0001ms, 0696ms total)
T5BD0 003:853 JLINK_IsHalted()  returns FALSE (0004ms, 0699ms total)
T5BD0 003:859 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0018ms, 0713ms total)
T5BD0 003:877 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0695ms total)
T5BD0 003:877 JLINK_ClrBPEx(BPHandle = 0x00000008)  returns 0x00 (0000ms, 0695ms total)
T5BD0 003:877 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0695ms total)
T5BD0 003:877 JLINK_WriteMem(0x200001E8, 0x0218 Bytes, ...) - Data: 00 BF 40 1C 28 4A 12 68 02 F4 00 31 19 B9 4F F6 ... -- CPU_WriteMem(536 bytes @ 0x200001E8)  returns 0x218 (0020ms, 0715ms total)
T5BD0 003:897 JLINK_WriteMem(0x20000400, 0x01E8 Bytes, ...) - Data: FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF ... -- CPU_WriteMem(488 bytes @ 0x20000400)  returns 0x1E8 (0019ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R0, 0x08000C00)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R1, 0x0000011C)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R2, 0x200001E8)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0734ms total)
T5BD0 003:916 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0001ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(R15 (PC), 0x2000013C)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000009 (0000ms, 0735ms total)
T5BD0 003:917 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0016ms, 0751ms total)
T5BD0 003:933 JLINK_IsHalted()  returns FALSE (0002ms, 0753ms total)
T5BD0 003:937 JLINK_IsHalted()  returns FALSE (0001ms, 0752ms total)
T5BD0 003:940 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0016ms, 0767ms total)
T5BD0 003:956 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0751ms total)
T5BD0 003:956 JLINK_ClrBPEx(BPHandle = 0x00000009)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R0, 0x00000002)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R1, 0x0000011C)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R2, 0x200001E8)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(R15 (PC), 0x20000070)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0751ms total)
T5BD0 003:957 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x0000000A (0000ms, 0751ms total)
T5BD0 003:957 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0016ms, 0767ms total)
T5BD0 003:973 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0017ms, 0784ms total)
T5BD0 003:990 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0767ms total)
T5BD0 003:990 JLINK_ClrBPEx(BPHandle = 0x0000000A)  returns 0x00 (0000ms, 0767ms total)
T5BD0 003:990 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0767ms total)
T5BD0 004:045 JLINK_WriteMem(0x20000000, 0x01E8 Bytes, ...) - Data: 00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(488 bytes @ 0x20000000)  returns 0x1E8 (0018ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R0, 0x08000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R2, 0x00000003)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(R15 (PC), 0x20000038)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0785ms total)
T5BD0 004:063 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x0000000B (0002ms, 0787ms total)
T5BD0 004:065 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0018ms, 0805ms total)
T5BD0 004:083 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0017ms, 0822ms total)
T5BD0 004:100 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_ClrBPEx(BPHandle = 0x0000000B)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R0, 0xFFFFFFFF)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R1, 0x08000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R2, 0x00000D1C)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R3, 0x04C11DB7)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0805ms total)
T5BD0 004:100 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0001ms, 0806ms total)
T5BD0 004:101 JLINK_WriteReg(R15 (PC), 0x20000002)  returns 0x00 (0000ms, 0806ms total)
T5BD0 004:101 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0806ms total)
T5BD0 004:101 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0806ms total)
T5BD0 004:101 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0806ms total)
T5BD0 004:101 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0806ms total)
T5BD0 004:101 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x0000000C (0000ms, 0806ms total)
T5BD0 004:101 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0016ms, 0822ms total)
T5BD0 004:117 JLINK_IsHalted()  returns FALSE (0002ms, 0824ms total)
T5BD0 004:124 JLINK_IsHalted()  returns FALSE (0002ms, 0824ms total)
T5BD0 004:128 JLINK_IsHalted()  returns FALSE (0002ms, 0824ms total)
T5BD0 004:131 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:134 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:137 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:140 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:143 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:146 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:149 JLINK_IsHalted()  returns FALSE (0002ms, 0824ms total)
T5BD0 004:152 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:157 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:160 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:162 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:166 JLINK_IsHalted()  returns FALSE (0000ms, 0822ms total)
T5BD0 004:168 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:171 JLINK_IsHalted()  returns FALSE (0001ms, 0823ms total)
T5BD0 004:174 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0017ms, 0839ms total)
T5BD0 004:191 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_ClrBPEx(BPHandle = 0x0000000C)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_ReadReg(R0)  returns 0x68E0B26B (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R0, 0x00000003)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R1, 0x08000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R2, 0x00000D1C)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R3, 0x04C11DB7)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R9, 0x200001E0)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R13 (SP), 0x20001000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(R15 (PC), 0x20000070)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(MSP, 0x20001000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(PSP, 0x20001000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_WriteReg(CFBP, 0x00000000)  returns 0x00 (0000ms, 0822ms total)
T5BD0 004:191 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x0000000D (0000ms, 0822ms total)
T5BD0 004:191 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) (0016ms, 0838ms total)
T5BD0 004:207 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0017ms, 0855ms total)
T5BD0 004:224 JLINK_ReadReg(R15 (PC))  returns 0x20000000 (0000ms, 0838ms total)
T5BD0 004:224 JLINK_ClrBPEx(BPHandle = 0x0000000D)  returns 0x00 (0000ms, 0838ms total)
T5BD0 004:224 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 0838ms total)
T5BD0 004:278 JLINK_WriteMemEx(0x20000000, 0x0002 Bytes, ..., Flags = 0x02000000) - Data: FE E7 -- CPU_WriteMem(2 bytes @ 0x20000000)  returns 0x02 (0001ms, 0839ms total)
T5BD0 004:279 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 0839ms total)
T5BD0 004:279 JLINK_Reset() -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET. >0x35 TIF>Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000)
 -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0095ms, 0934ms total)
T5BD0 004:374 JLINK_Go() -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0011ms, 0945ms total)
T5BD0 004:394 JLINK_Close() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000201C) >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF>
 >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> (0031ms, 0976ms total)
T5BD0 004:394  (0031ms, 0976ms total)
T5BD0 004:394 Closed (0031ms, 0976ms total)
